 **PVR Tech Safety Checklist**

Driver Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Sled Number: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Sled Year, Make, Model, Engine Size (cc): \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Classes Running: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

|  |  |
| --- | --- |
| **Safety Inspection:****Helmet** | X if Comply |
| 1. Snell 2015 or European Standard 22.05:  | \_\_\_\_\_\_\_\_ |
| 2.Must be Minimum 75% Orange  | \_\_\_\_\_\_\_\_ |
| 3. raciever  | \_\_\_\_\_\_\_\_ |
| 4.isr number  | \_\_\_\_\_\_\_\_ |
| **Safe Jacket**  | \_\_\_\_\_\_\_\_ |
| **Shin Guards** **Back of Racers Jacket** | \_\_\_\_\_\_\_\_ |
| 1. Must be 144 sq. inches Orange  | \_\_\_\_\_\_\_\_ |
| 2. Number Must be Minimum 6" Tall & Clearly Visible  | \_\_\_\_\_\_\_\_ |
| 3. Number Must Match Number on Sled  | \_\_\_\_\_\_\_\_ |
| **Safety Tether - Must Be Operational** **Tail Light** | \_\_\_\_\_\_\_\_ |
| 1. Visible/Bright - LED or 1157 Bulb on Bright (Brake) Element  | \_\_\_\_\_\_\_\_ |
| 2. Minimum Size 2X4 inches  | \_\_\_\_\_\_\_\_ |
| **Headlight - Removed or Taped Over**  | \_\_\_\_\_\_\_\_ |
| **Brake - Must Be Operational** **Clutch Cover** | \_\_\_\_\_\_\_\_ |
| 1.Must Be .060" Thick 6061T6 Aluminum or Equivalent Steel  | \_\_\_\_\_\_\_\_ |
| 2.Must Be Covered With 6" Wide Belting  | \_\_\_\_\_\_\_\_ |
| 3. Must Be Separate From Cowl  | \_\_\_\_\_\_\_\_ |
| 4. Must Cover to Center or Below Primary and Secondary Bolts **Tunnel**1. Rear of Tunnel Enclosed With Aluminum or Steel in Comparable  | \_\_\_\_\_\_\_\_ |
| Strength of Tunnel Material2. Must Cover Rear and Sides of Tunnel Extending Forward to Rear  | \_\_\_\_\_\_\_\_ |
| Suspension Mounting Bolts3. Bottom of Enclosure Shall Not be Higher Than 1" Above Center of Rear  | \_\_\_\_\_\_\_\_ |
| Axle With Driver in Place | \_\_\_\_\_\_\_\_ |
| **Snow Flap - Must Touch Ground W/Driver on Sled. Pinned or Chained.** | \_\_\_\_\_\_\_\_ |
| **Handle Bars, Steering & Skis Are Functional & Not Loose** | \_\_\_\_\_\_\_\_ |
| **Hood, Fuel Tank & Seat Secure****Track Stand - Rear & Side Guards Extending**  | \_\_\_\_\_\_\_\_ |
| **From Ground to Above Rear Running Boards and Forward to Rear Axle** | \_\_\_\_\_\_\_\_ |
|  |  |

Driver (Signature) \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Inspection Performed By (Signature) \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_\_\_\_\_\_\_

Date PVR Tech Sticker Issued and Applied to Sled: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Last Revision 12/5/2019